# Deployment

The end-to-end deployment workflow for UB-EDGE One lives in the setup guide:

- [Flash OpenWrt and install the UB-EDGE image](teltonika_flash_guide.md#flash-the-openwrt-factory-image-teltonika-rutx50)
- [Post-flash controller checklist](teltonika_flash_guide.md#post-flash-controller-checklist)
- [Deployment overview and field upgrade pattern](teltonika_flash_guide.md#deployment-overview)

Use this page for operations-specific addenda—automation hooks, customer-specific variations, or lessons learned that complement (but do not duplicate) the core guide.

## Outstanding Gaps
- Placeholder: Document automation opportunities (ansible playbooks, CI hooks) for deployment.
- Placeholder: Capture customer-specific variations that need separate runbooks.
## Deployment Scenarios
- Placeholder: Distinguish between greenfield install, expansion, and upgrade paths.
- Placeholder: Document prerequisites (site survey, power availability, connectivity assumptions).

## Preparation Checklist
- Placeholder: Create packing list, firmware versions to preload, and SIM activation steps.
- Placeholder: Capture stakeholder communications required before site arrival.

## On-Site Procedure
- Placeholder: Outline step-by-step install (mounting hardware, cabling, initial power-up) with responsible roles.
- Placeholder: Include validation checks (signal strength, throughput tests) and how to record results.

## Post-Deployment Verification
- Placeholder: Document remote access enablement, monitoring onboarding, and customer training.
- Placeholder: Define sign-off criteria and handover documentation requirements.

## Rollback & Contingency
- Placeholder: Provide plan for reverting to previous firmware/configurations if deployment fails.
- Placeholder: Note spare hardware strategy and escalation contacts.
