# System: CCR-Aachen  

- [[#General Information|General Information]]
- [[#Hardware Components|Hardware Components]]
- [[#Maintenance|Maintenance]]
- [[#Access & Credentials|Access & Credentials]]
- [[#References|References]]
- [[#Outstanding Data|Outstanding Data]]

## General Information
- **Location:** Aachen  
- **Address:** Center Construction Robotics, Campus-Boulevard 79, 52074 Aachen  
- **Responsible Person:** Lukas  
- **Date of Installation:** 16.10.2025
- **Purpose:** Testing  
- **SIM:** O2 XXX  

## Hardware Components

| Component            | Serial No.   | MAC Address   | WireGuard IP | OS/Firmware | Notes                     |
|----------------------|--------------|---------------|--------------|-------------|---------------------------|
| Teltonika RUTX50     | 6006511637   | 209727798ECE  | 192.168.201.44 | UB 4b0111e3 15.10.2025  |            |
| QuWireless QuCAM50   | 62194        |               |              |             | 3 x PoE, 1 x external SIM |
| NWA55AXE             | S241843005605  | F44D5CFD9DEC |              |             |                           |
| NWA55AXE             |              |               |              |             |                           |
| NWA55AXE             |              |               |              |             |                           |

## Maintenance
- **Known issues:**  
- **Special config:** Is to be extended for bonding  

- Placeholder: Add planned installation timeline and prerequisites for bonding setup.
- Placeholder: Record remote monitoring status and responsible engineer.

## Access & Credentials

- UB User: admin PW: Uniberg123!
- Teltonika:
-- SSID RUT_8ED0/1_2/5G
-- WIFI: Xs10Zja6
-- Management: Rq3*^7Je

## Contact
zoecklein@construction-robotics.de

- Placeholder: Capture site photos, layout diagrams, and contact list.

# Notes

## [[Lukas]] 16.10.2025 vor Ort in Aachen

Ich fasse mal die bisherigen Findings zusammen:

- Flashen mit Anleitung klappt gut - hab noch nen kleinen Typo in einem Command (böses Leerzeichen) gefunden - will fix 
- 5s springbug in UI gefunden - Bassem weiß schon Bescheid und fixed
- UI ist noch voll mit Werten die entweder statisch sind oder unsinning - sollten wir fixen!

Mit der O2 Karte bekommen wir hier ca 80-100Mbits Downlink (schwankt was) Erkentnisse zur Platzierung:

1. Platzierung Außen

- Baufeld gut (bis ans Ende noch bis ca 40 Mbits)
- Containers sehr gut (alle Arbeitsplätze zwischen 50-80 Mbits)
- Klo nur gut mit offener Tür

2. Platzierung Innen am Fenster

- Baufeld eher meh (am Ende ca 20 Mbits aber low fps und problems)
- Containers - im Container wo es steht 90 Mbits (fast perfekt), im Container drüber und schräg gegenüber mies (10-20Mbits, problemos)
- Klo sowieso nur mit offener Tür

Interpretation:

- Für den eigentlichen Backhaul macht Innen vs Außen kaum unterschied wenn gut am Fenster platziert
- Für das Wifi ist im Container platzieren scheisse wenn man nicht im selben raum ist - because of obvious reasons